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1. Introduction to Optical Fibers 

Optical communication is one of the oldest methods of communicating.
The principle of optical communication is to use the light energy to send a message from one point to another. By light energy we mean the infra-red, visible and ultra-violet regions of the electromagnetic spectrum.
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The realization of an optical communication system involves a light source, modulator, (transmitting lens), transmission medium, a light detector, receiver, (repeater), transmitter and receiver electronics, processing.

The simplest system is a man turning a flashlamp on and off and another person watching him.

[image: image3.png]On-off switch

1~ transmission > Eye
= medium

Flash lamp




Here the light source is the flash lamp, turning the switch on and off corresponds to modulation, the transmission medium is the atmosphere, the eye is the detector, human brain is the processor. The data rate we provide depens on how fast we can turn the flashlamp on and off.

The factors to be considered in such a simple system are:

· The overall cost of the system,
· Frequency of the light source (carrier frequency),
· Frequency should match the operating frequency of the detector,
· Bandwidth of the light source (causes dispersion, i.e., brodening of the received pulse),
· Modulation rate (bir rate with unit bit/second). Limited by the switching electronics. Modulation rate determines the rate of information, i.e., what amount of data can be sent in one second, 
· Medium losses (attenuation). Free space loss, absorption and scattering,
· Dispersion in the medium, i.e., widening of the received pulse which results in the reduction of the bit rate that can be used,

· Detector operating frequency that should match the source carrier frequency,
· Detector response time which should be fast enough to accomodate the modulation rate
      If the distance is long then a person will be in the middle to convey the message (repeater).

     Types of optical communication systems:

a) Free space systems. Space-to-space satellite links. (Unguided).

b) Atmospheric systems. Horizontal terrestrial links, earth to satellite links, satellite to earth links. (FSO, Free Space Optics) (Unguided)  
c) Oceanic (underwater) systems. Guided systems with optical fiber and unguided wireless systems.

d) Optical fiber systems under and above the ground. Guided.
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     Advantages of optical fiber systems over the coaxial twisted wire systems:
· High repeater spacing possible (100 km or more),

· Potential of extremely high data bit rate. Terabit per second = 1012 bps or more. Around million million TV channels or billions of telephone channels or Tbps internet traffic,

· Low weight,

· Low cost,

· No electromagnetic interference (EMI),

· High security. Tapping of the signal by unauthorized persons is not possible. 

      Most optical fiber systems utilize PCM (Pulse Code Modulation).
     [image: image5.emf]
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Basic optical communication system architecture

       Block diagram:
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      Main components of optical fiber systems:

1. The optical source: LED (semiconductor), laser diode (semiconductor),
2. A means of modulating the optical output from the source with the signal to be transmitted (internal modulation),

3. The transmission medium: Step index fibers (single mode, multimode),graded index fibers (multimode)

4. The photodetector which converts the received the received optical power back into an electrical signal. Pin (semiconductor), avalanche (semiconductor),

5. Electronic amplification and signal processing required to recover the signal and present it in a form suitable to use.

6. Connectors (source to fiber, fiber to fiber, fiber to photo detector) and splicing (fiber to fiber).
2.    Propagation of Light in Optical Fibers
Total internal reflection
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     At the critical angle      [image: image9.png]



From Snell’s Law,  
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For 
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, total internal reflection occurs with no losses at the boundary and the light ray is totally reflected at the interface.

i.e., when 
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 is increased, there appears an angle 
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 (called the critical angle) where the refracted ray becomes parallel to the interface. If  
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 is further increased (i.e., for 
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) all the energy contained within the incident light ray is reflected back into the same medium (i.e., the core) so no energy is refracted into the second medium. Thus, no energy is lost. This phenomenon is called total internal reflection.    

Considering a cylindrical glass fiber where 
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The ray enters the end face of the fiber from the outside (refractive index of air =na=1).
For 
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, total internal reflections will occur and the ray will propagate along the fiber (in the core) without loosing energy. 

Writing Snell’s Law at the air to fiber boundary
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For 
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Inside the core, 
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So 
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Thus, 
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Let 
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 The greater the value of 
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, the greater is the proportion of the light incident onto the end face that can be collected by the fiber and be propagated by internel reflection.
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 is defined as the numerical aperture (NA) which is a measure of light gathering power (acceptance cone) of the optical fiber. For 
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Conclusion is that in order for the fiber to guide the light, angle of incidence to fiber (
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) should be less than 
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If 
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, then refraction will occur at the core-cladding interface and the optical power is lost.

3.    Mode Structure in Optical Fibers 
Waveguide equations, wave and ray optics
Propagation of light within the fiber can be formulated using either the wave optics or the ray optics.

In wave optics, field theory is used to derive a wave equation in terms of the longitudinal components of the fields in the guide. Then using the transformation equation (derived using Maxwell’s equations) the transverse components of the fields are found in terms of the longitudinal components. Various solutions of the wave equation determine the propagation of the modes within the fiber.

In ray optics, propagation of the modes are presented by rays following different paths.   

Basic waveguide equations; Wave optics

Consider the waveguide structure
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· Assume that the propagation is in z-direction with a longitudinal propagation constant 
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 (i.e., 
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 is the longitudinal component of the propagation vector 
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· Assume that the permittivity 
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 does not depend on z but can vary with x and y. However, it is assumed to vary small amounts over the region of the wavelength so 
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 is taken as constant. 

The fields in a waveguide can be written as
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 where for 
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Here 
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 = propagation constant in z-direction is to be determined.

Using the Maxwell’s equations
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From Eq. (2),  
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Substituting Eq. (5) into Eq. (4) and writing in component form 
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To express 
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Multiplying Eq. (8) by 
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where 
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Similarly from Eqs. (6b) and (7b) we obtain
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From  
[image: image73.wmf]z

yx

E

jEjH

y

bwm

¶

+=-

¶

 and 
[image: image74.wmf]z

xy

H

jHjE

x

bwe

¶

--=

¶

, we obtain 
[image: image75.wmf]2

zz

x

jHE

H

xy

bwe

k

æö

¶¶

=--

ç÷

¶¶

èø


From 
[image: image76.wmf]z

xy

E

jEjH

x

bwm

¶

--=-

¶

 and 
[image: image77.wmf]z

yx

H

jHjE

y

bwe

¶

+=

¶

, we obtain 
[image: image78.wmf]2

zz

y

jHE

H

yx

bwe

k

æö

¶¶

=-+

ç÷

¶¶

èø


[image: image79.emf]
[image: image80.emf]
[image: image81.emf]
[image: image82.emf]
[image: image83.emf]
[image: image84.emf]
[image: image85.emf]
[image: image86.emf]
[image: image87.png]ST JF(r) N )
. JY‘— ar +<KZ—F>FU‘)=O {5

/

This s 2 form o)(L Bessells e ation, The soluddon.
shoold  have  the g_a\kog)\vxﬂ ?m?@:\ﬂe_g . t
(D e Liedd i He e push Lo Sk ol oo [
QLL) Caddog  faeld must  have  an %cv\wkuj ‘
decaging  Lehavier st large  distences  fropw the
center of the Liber :

TThe proper  soloken Lr & 0w
ATvQKYﬁeT‘\Ws , r<a

N‘Tﬂ
Il
(x’L/\
<
o
“
<
ASH
|
l
Q

(@ Hv<53f _ r>3
Sidarly
- B 3 (%) ewgé , =3 N !
H, = { 0 NN " = i
b oo\ P , T >a
: D Hy Grr)e g
|

w herve I) s Lhe Ressel ;MCTLLM o—(,— order Y
HQ) " “ MO&\‘LQJ Backel {—uﬂ\C‘ﬁD‘h D~)(- He

Dirst Yind aL order V
’ 5B CGD are ytbrewn constants

Trow Maxwells Q%MQ.‘L\M Br, &, W, Wy \u;\ e
‘ are  fownd as (Lo tremvese fells for r<d)
e ‘ /7%:SV(HB —\j\)ﬁij

g, = =% [h3K 3 (k) + E(gv\/(\v,@,‘ymw}k

s V\Z
o =
By = 3 [p AT (k) -RupB Y Wﬁeﬂ;
®: L _ Ve 9
oo _i ,',~,,ue‘\) AJ_\,(KF) +Kp BRI (Kr)lgj @;
- J 7 (k3
Hg= - [Kwe AT/ (k) +3pFRY T e |




[image: image88.emf]
[image: image89.emf]
[image: image90.png]-t e

0 .
where W (jv O{a) O : _Hv‘) (53’33 :
S e 3 s e
E ERve ,,U@ yuzx V(KQB‘T}Z \)(jx> Y H\’Cﬁﬂ‘
, A ~ ' _ B |
\ - ‘
o M CA T R -HVO’(W;}!
—IWE v iuN y B W 0L N TYR e
K\‘ T (\.(u) : Fj\/(h)‘[ % i) Jm\/ QWHV (:)Z,/g)

Nondrvial  seluton Lo (D gves
dedemonant  of (W) =\w| =0
o W , ,
lwi=0  gives e eljenvalve” on iﬂ‘,di characiericlc

\)\%‘\r\w\, 0!1 ‘Q/‘E. anegmuie_
%C\Aa\faﬁ_i&w_i—&c e gl*m can.  be Qewmsi as

3 23, (¥ H
S SCE m) T e
— [\) EL-—i “%\42 } )
= SNy — D
As deledric 5\350 wa\/a%wli& Q and
= q(fﬁm") Yod circle wll dedermane L Lo

modes "fr e :\sz? e 1 ber ‘ .
Loun (
_— AB Q/D W_JMV 5 AN LQ -paJLQ 7[w:rw\ )

) we. -wal e characterche i—a)\x&%m.ﬁar{),{

—c des when J=o E'(E:D M?.r\&\oy\a\ r.gqj
%M v J=0 Uy =0 (cromes Hhe asey
ne {(Ha s te dedermining ?\d‘g <bew Cays
Ex (& . . . 2 E J+o




[image: image91.emf]
[image: image92.png]N = of

©
A
_Fhé,g

ao
e M

——
m
d .
=
e o
, K

o

‘uw

=

lo

1L V< z.es e
Sgle wole fles
s Todal no.ol wodesiNin 2

VY omber oLt Flan
V= Kﬂa:;?)ém

= 2T
L a@%\) N is large

. ‘
N=kV o 2
w2

shep \v\ie)’\ Ller =




[image: image93.emf]
[image: image94.png]Graded Todex ?ijber

Refrackive index pro Lie

//' B ‘ Y |
[ . fl-es Gy T

\\ \V,v; o Va2 \

VAN ( |—2A> s Za i ‘
A= niefs !

o

2a2 ~— O/

Tt

5
3
A

—_ ,Bazné_wti'u'\ 0—§~ 3Ta,e‘Lei maex g/\&:&(‘ ~ FOO MH’}AM -
3 eha-ka,

shenns for ehop onfer | Laduittl o[ e filer << 100 Mk,

Ray oplics analysis  of +he grac\eéfimlex Liler

'Raxi ‘%rajecjmw will ke -)CDUV\A )05 \vwg
e “uii Ey&&,\b%_\)\)(i{{,\oy{: iw-‘f\/a‘hem wa  wrbi He Parai

Iy — O

T, 27

az

e velvacive wdex  doesnst  chamse wed &

Thas Bh o Usieg s T @ anl wderabiyg
Lo
rz AQ’ o consTarT AQ’ . .
dz =9 — d= 'r—z e 2




[image: image95.emf]
[image: image96.emf]
[image: image97.emf]
4.    Optical Fiber Communications Link Design
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5.    Attenuation in Optical Fibers, Power Budget Analysis 
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Transmisssion windows (lowest attenuation at 
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 has low attenuation, too. 
6.    Dispersion in Optical Fiber Communications
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7.    Optical Sources and Detectors used in Optical Fiber Systems  
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8.    Optical Fiber Transmitter  
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PULSE CODE MODULATION (PCM)
PCM is the conversion of an analog signal into a 2n-digit binary code. 
[image: image137.emf]
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An analog signal is placed on the input of a sample and hold. 
The sample and hold circuit is used to “capture” the analog voltage long enough for the conversion to take place.
The output of the sample and hold circuit is fed into the analog-to-digital converter (A/D).
An A/D converter operates by taking periodic discrete samples of an analog signal at a specific point in time and converting it to a 2n-bit binary number. 
For example, an 8-bit A/D converts an analog voltage into a binary number with 28 discrete levels (between 0 and 255). 
For an analog voltage to be successfully converted, it must be sampled at a rate at least twice its maximum frequency. This is known as the Nyquist sampling rate. 
An example of this is the process that takes place in the telephone system. A standard telephone has a bandwidth of 4 kHz. When you speak into the telephone, your 4-kHz bandwidth voice signal is sampled at twice the 4-kHz frequency or 8 kHz. Each sample is then converted to an 8-bit binary number. This occurs 8000 times per second. Thus, if we multiply 8 k samples/s × 8 bits/sample = 64 kbits/s, we get the standard bit rate for a single voice channel which is 64 kbits/s. 
The output of the A/D converter is then fed into a driver circuit that contains the appropriate circuitry to turn the light source on and off. 
The process of turning the light source on and off is known as modulation.

The light then travels through the fiber and is received by a photodetector that converts the optical signal into an electrical current. 
A typical photodetector generates a current that is in the micro- or nanoamp range, so amplification and/or signal reshaping is often required. 
Once the digital signal has been reconstructed, it is converted back into an analog signal using a device called a digital-to-analog converter or DAC. 
A digital storage device or buffer may be used to temporarily store the digital codes during the conversion process. 
The DAC accepts an n-bit digital number and outputs a continuous series of discrete voltage “steps.” 
All that is needed to smooth the stair-step voltage out is a simple low-pass filter with its cutoff frequency set at the maximum signal frequency.
DIGITAL ENCODING SCHEMES

Signal format is an important consideration in evaluating the performance of a fiber optic system..

The signal format directly affects the detection of the transmitted signals.
The accuracy of the reproduced signal depends on the intensity of the received signal, the speed and linearity of the receiver, and the noise levels of the transmitted and received signal.
Many coding schemes are used in digital communication systems, each with its own benefits and drawbacks.

The most common encoding schemes are the return-to-zero (RZ) and non-return-to-zero (NRZ).

The NRZ encoding scheme, for example, requires only one transition per symbol, whereas RZ format requires two transitions for each data bit. 
This implies that the required bandwidth for RZ must be twice that of NRZ. This is not to say that one is better than the other. 
Depending on the application, any of the code formats may be more appropriate than the others.
For example, in synchronous transmission systems in which large amounts of data are to be sent, clock synchronization between the transmitter and receiver must be ensured. In this case Manchester encoding is used. 
The transmitter clock is embedded in the data. The receiver clock is derived from the guaranteed transition in the middle of each bit. 

[image: image139.png]DatajOfOfOl1l00lo 1110t l1]1]

Clock LI ILLririrrrirm
[ T A I O O O

;7N p I I S

Manchester —J LT LI L1 LI LML

Symbols . Duty Factor
Format vyt SeFClocking o O
NRZ 1 No 0-100
RZ 2 No 0-50
Manchester
(Biphase L) 2 Yes 50





Digital systems are analyzed on the basis of rise time rather than on bandwidth. 
The rise time of a signal is defined as the time required for the signal to change from 10% to 90% of its maximum value.
The system rise time is determined by the data rate and code format.

Depending on which code format is used, the number of transitions required to represent the transmitted data may limit the overall data rate of the system.
The system rise time depends on the combined rise time characteristics of the individual system components.
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(a) represents a signal with adequate rise time. Even though the pulses are somewhat rounded on the edges, the signal is still detectable.
In (b) however, the transmitted signal takes too long to respond to the input signal. 
The effect is the below figurewhere at high data rates, the rise time limitations cause the data to be distorted and thus lost.
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To avoid this distortion, an acceptable criterion is to require that a system have a rise time ts of no more than 70% of the pulse width Tp, ts ≤ 0.7 Tp  
For an RZ, Tp takes half the bit time T so that ts ≤ 0.7 T/2 or

ts ≤ 0.35/Br where Br = 1/T is the system bit rate.

For an NRZ format, Tp = T and thus ts ≤ 0.7/Br 
RZ transmission requires a larger-bandwidth system.
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9.    Optical Receiver Systems
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10.  Introduction to Free Space Optics (FSO) Systems 

Based on their transmission range, WOC (Wireless Optical Communication) can be classified into five broad categories:

(i) Ultrashort-range WOC – used in chip-to-chip communication or all optical lab-on-a-chip system.

(ii) Short-rangeWOC – used in wireless body area networks (WBANs) or wireless personal area networks (WPANs).

(iii) Medium-range WOC – used in indoor IR or visible light communication (VLC) for wireless local area networks (WLANs) and inter-vehicular and vehicle-to-infrastructure communications.

(iv) Long-range WOC – used in terrestrial communication between two buildings or metro area extensions.

(v) Ultra-long-range WOC – used in ground-to-satellite/satellite-to-ground or inter-satellite link or deep space missions.
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Block diagram of WOC
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FSO applications:

• Telecommunication and computer networking

• Point-to-point LOS links

• Temporary network installation for events or other purpose as disaster recovery

• For communications between spacecraft, including elements of satellite constellation 

• Security applications

• Military application: (its potential for low electromagnetic emanation when transferring sensitive data for air forces)

• Metro network extensions: carriers can deploy FSO to extend existing metropolitan area fiber rings, to connect new networks, and, in their core infrastructure, to complete SONET rings.

• Enterprise connectivity: the ease with which FSO links can be installed makes them a natural for interconnecting local area network segments that are housed in buildings separated by public streets or other right-of-way property.

• Fiber backup: FSO may also be deployed in redundant links to backup fiber in place of a second fiber link.

• Backhaul: FSO can be used to carry cellular telephone traffic from antenna towers back to facilities wired into the public switched telephone network.

• Service acceleration: FSO can be also used to provide instant service to fiber-optic customers while their fiber infrastructure is being laid.

• Last-Mile access: In today’s cities, more than 95% of the buildings do not have access to the fiber optic infrastructure due to the development of communication systems after the metropolitan areas. FSO technology seems a promising solution to the connection of endusers to the service providers or to other existing networks. Moreover, FSO provides highspeed connection up to Gbps, which is far more beyond the alternative systems.
FSO Advantages:

• Long distance up to 8 km.

• High bit rates speed rates: the high bandwidth capability of the fiber optic of 2.5 Gbps to 10 Gbps achieved with dense wavelength division multiplexing (DWDM). Modern systems can handle up to 160 signals and can thus expand a basic 10 Gbit/s system over a signal fiber pair to over 1.6 Tbit/s.

• Immunity from electromagnetic interference: secure cannot be detected with RF meter or spectrum analyzer, very narrow and directional beams

• Invisible and eye safe, no health hazards so even a butterfly can fly unscathed through a beam

• Low bit error rates (BER)

• Absence of side lobes

• Deployment of FSO systems quickly and easily

• Low maintenance (Practical)

• Lower costs as compared to fiber networks (FSO costs are as low as 1/5 of fiber network costs).

• License-free long-range operation (in contrast with radio communication)

FSO disadvantages:

For terrestrial applications, the principal limiting factors are beam dispersion, atmospheric absorption, rain, fog, snow, interference from background light sources (including the sun), shadowing, pointing stability in wind, and pollution.
Atmospheric effects:

Transmitted power of the emitted signal is highly affected by scattering, absorption and turbulence.

Attenuation is the result of absorption and scattering by molecules and particles (aerosols) suspended in the atmosphere. 

Distortion, on the other hand, is caused by atmospheric turbulence due to random index of refraction fluctuations. 

Attenuation affects the mean value of the received signal in an optical link whereas distortion results in variation of the signal around the mean.

Aerosols:

Aerosols are particles suspended in the atmosphere with different concentrations. Each aerosol cause absorption and scattering. 

They have diverse nature, shape, and size. Aerosols can vary in distribution, constituents, and concentration. As a result, the interaction between aerosols and light can have a large dynamic, in

terms of wavelength range of interest and magnitude of the atmospheric scattering itself. Some aerosols are rain, smoke, fog, snow, desert dust particles, human-made industrial particulates, maritime droplets. 

Aerosol scattering are explained by Mie scattering theory because the sizes of aerosols are comparable to or larger than the wavelength of the optical communications.
Transmitted optical beams in free space are attenuated most by the fog and haze droplets mainly due to dominance of Mie scattering and absorption effects in the wavelength band of interest in FSO (0.5 μ m – 2 μ m). 
The Mie scattering coefficient is 
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 is the Mie scattering cross-section in km2  and  
[image: image156.wmf]a
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 is the number density of air particles in 1/km3.
An aerosol’s concentration, composition and dimension distribution vary temporally and spatially varying, so it is difficult to predict attenuation by aerosols. Although their concentration is closely related to the optical visibility, there is no single particle dimension distribution for a given visibility. Due to the fact that the visibility is an easily obtainable parameter,either from airport or weather data, the scattering coefficient 
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where 
[image: image159.wmf]V

 is the visibility (Visual Range) in km, 
[image: image160.wmf]l

 is the incident laser beam wavelength μm, i is the size distribution of the scattering particles which typically varies from 0.7 to 1.6 corresponding to visibility conditions from poor to excellent.

Also the absorption coefficient of the aerosol 
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 is found and the atmospheric transmittance due to an aerosol is found to be 
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where the total attenuation due to an aerosol is 
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 and L is the link distance, i.e., the distance between from the transmitter and the receiver.

Thus, the total attenuation due to aerosols is found by evaluating the scattering and absorption coefficients of each aerosol present in the FSO link and by adding them to find 
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Molecules:

There are more than 40 different molecules in the atmosphere, e.g., nitrogen, hydrogen, carbon dioxide, ... etc. Each of these molecules cause scattering and absortion. 
Rayleigh (molecular) scattering refers to scattering by molecular and atmospheric gases of sizes much less than the incident light wavelength. The Rayleigh scattering coefficient is given by 
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where 
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  is the Rayleigh scattering cross-section in km2,
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 is the number density of air molecules in 1 /km3. 

Rayleigh scattering cross section is inversely proportional to fourth power of the wavelength

of incident beam (λ-4) as
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where n is the index of refraction, λ is the incident light wavelength in m, N  is the volumetric density of the molecules in 1 /km3.

The result is that Rayleigh scattering is negligible in the infrared waveband because Rayleigh scattering is primarily significant in the ultraviolet to visible wave range.
Also the absorption coefficient of the molecule 
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 is found and the atmospheric transmittance attenuation due to a molecule is found to be 
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where the total attenuation due to a molecule is 
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 and L is the link distance, i.e., the distance between from the transmitter and the receiver.

Thus, the total attenuation due to molecules is found by evaluating the scattering and absorption coefficients of each molecule present in the FSO link and by adding them to find 
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Turbulence

Clear air turbulence phenomena affect the propagation of optical beam by both spatial and temporal random fluctuations of refractive index due to temperature, pressure, and wind variations along the optical propagation path.

Atmospheric turbulence primary causes phase shifts of the propagating optical signals resulting in distortions in the wave front. 

These distortions, referred to as optical aberrations, also cause intensity distortions, referred to as scintillation. 

Moisture, aerosols, temperature and pressure changes produce refractive index variations in the air by causing random variations in density. 

These variations are referred to as eddies and have a lens effect on light passing through them. 

When the light beam wave passes through these eddies, parts of it are refracted randomly causing a distorted wave front with the combined effects of variation of intensity across the wave front and warping of the isophase surface.

As the result, turbulence causes scattering 
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i.e., the overall total attenuation due to aerosols, molecules and turbulence is found by 
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Other effects of turbulence: 
· Beam wander
[image: image180.emf]
· Beam spread: Beam size at the receiver is increased further on top of free space diffraction.
· Intensity fluctuations: Intensity at the receiver fluctuates in time and space.
11.  Propagation of Light in FSO
Free-Space Propagation of Gaussian-Beam Waves
The mathematical description of a propagating wave involves a field.

Basically, a field 
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 is a function of space R = (x, y, z) and time t that satisfies a partial differential equation. 

In the case of electromagnetic radiation, the field may be a transverse electromagnetic (TEM) wave, whereas for acoustic waves the field may represent a pressure wave. 

The governing equation in most cases is the wave equation
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where 
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 is the speed of the propagating wave which is light and 
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  is the Laplacian operator defined in rectangular coordinates by
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If we assume that time variations in the field are sinusoidal (i.e., a monochromatic wave), then we look for solutions  of the form 
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 is the angular frequency and 
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 is the complex amplitude of the wave which is the spatial field. 
The substitution of this solution form into the wave equation leads to the time-independent reduced wave equation (or Helmholtz equation)
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 where k is the optical wave number related to the optical wavelength 
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For optical wave propagation, Helmholtz equation can be further reduced to what is called the paraxial wave equation. 

Let us assume the beam originates in the plane at z=0 and propagates along the positive z-axis. If we also assume the free-space optical field at any point along the propagation path remains rotationally symmetric, then it can be expressed as a function of 
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 and z.

Thus, the reduced wave equation in cylindrical coordinates can be written as
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Paraxial approximation can be made when the propagation distance of an optical wave along the z-axis is much greater than the transverse spreading of the wave. 
[image: image194.emf]
If R = (r, z) and S = (s, z) denote two points in space with r and s transverse to the propagation axis, then the distance between such points is
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If the transverse distance is much smaller than the longitudinal propagation distance between the points, then the second factor can be expanded in a binomial series to obtain
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  which is known as the paraxial approximation.
The complex amplitude at propagation distance z from the source is given by Huygens-Fresnel integral as
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where 
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 is the optical wave at the source plane and 
[image: image199.wmf](

)

,;

Gz

sr

 is the free-space Green’s function which can be expressed under the paraxial approximation as
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The complex amplitude of the Gaussian-beam wave at the source plane z=0 is
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where A is the amplitude at the origin, 
[image: image202.wmf]22
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 is radial distance from the beam center line and 
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. It is assumed that the transmitting aperture is located in the plane z=0 and the amplitude distribution  in this plane is Gaussian with effective beam radius (spot size) W0 in meters, which denotes the radius at which the field amplitude falls to 1/e of that on the beam axis as shown below for A=1
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Additionally, the phase front is taken to be parabolic with radius of curvature 
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 in meters. The particular cases 
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 correspond to collimated, convergent, and divergent beam forms, respectively

[image: image207.emf]
Thus, for the Gaussian beam, Huygens-Fresnel integral becomes
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Changing the integration to polar coordinated where 
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 and rearranging  


[image: image210.wmf](

)

(

)

2

222

0

00

,expexpcosexp1

222

Aikikikik

Uzikzrrsizssdds

zzzz

p

qaq

p

¥

æöæöéù

=-+-+

ç÷ç÷

êú

èøèøëû

òò

r


Performing the integrations, the electric field at the receiver is found as
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The intensity at the receiver is 
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12.  FSO Link Design 

The ability for an optical link to deliver the signal power to the receiver is

governed by the link equation

[image: image213.wmf]22

4

4

TR

RTTATPatmpolRPR

AA

PPLLLL

z

p

hhh

lp

æöæö

=

ç÷ç÷

èøèø


where
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P

 is the total signal power at the input to the receiver. For the uplink, this is defined at the input to the optical detector. For the downlink, the receive signal power is defined at the input to the receive optical detector,
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 is the transmit optical power at the transmit interface,
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 is the transmit optics efficiency,

[image: image217.wmf]A

h

 is the aperture illumination efficiency of the transmitter lens,
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 is the wavelength,
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 is the aperture area,
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 is the transmitter pointing loss, defined as the ratio of power radiated in the direction of receiver to the peak radiated power. If the transmitter is directly pointed at the receiver, the pointing loss is 0 dB,
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 is the fractional loss due to absorption of the medium (e.g., earth atmosphere),
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 is the fractional signal loss due to mismatch of the transmitting and receiving polarization patterns,
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 is the receiver pointing loss, defined as the ratio of receiving lens gain in the direction of the transmittting lens to the peak receiving lens gain,
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 is the receive aperture area,
z is the link distance,
the term 
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 is the fraction of power that is collected by the receiving aperture if the transmitter is an isotropic radiator.
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 is the receiving optics collecting efficiency, defined as the fraction of optical power at the receiving aperture that is collected within the field of view of the receive detector.

Thus, the receive signal power can be improved by the following:

1) Increasing the transmit power. The most straightforward method of improving the receive signal power is to increase the power at the transmitter since the receive power scales linearly with the transmit power. However, increasing the transmit power also increases the overall system power consumption which, for a deep-space mission, is typically at a premium. Furthermore, the increased power consumption can lead to thermal management issues (increased radiator size and hence mass) for the host spacecraft, as well as reliability concerns.

2) Increasing the transmit aperture. This effectively reduces the transmit beamwidth and hence improves the power delivery efficiency. However, the pointing and tracking of the narrow downlink becomes increasingly more difficult with a narrower downlink. Furthermore, the aperture size is highly correlated with the mass of the transmit terminal and hence cannot be increased indefinitely.

3) Reducing the operating wavelength. Reducing the operating wavelength reduces the diffraction loss of the signal (i.e., reduces the transmit beamwidth). However, the wavelength selection is strongly constrained by the available laser technology, as well as considerations on the receiver sensitivity and detector technology. Furthermore, the transmittance of the atmosphere also depends on the wavelength, as well as the amount of sky background irradiance.

4) Increasing the receiver aperture area. Since the receive signal power scales linearly with the receive aperture area, increasing the receiver aperture area is a relatively simple way to improve the system performance. However, for daytime operations of a receiver inside the Earth’s atmosphere, the amount of background noise collected also increases with increasing receiver aperture, and the effective performance improvement does not always scale linearly with increasing aperture area.

5) Reduced pointing loss. Reducing the pointing loss improves the overall signal energy and also reduces the point-induced signal power fluctuation.

6) Improving the overall efficiency, including transmit and receive optical loss, and polarization mismatch losses. This generally requires attention to the optical design. Of particular attention is the transmit optics design. The transmit aperture illumination efficiency, 
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, depends on the phase and intensity distribution over the aperture. For the general case of a transmit aperture being illuminated by a Gaussian beam, the aperture illumination efficiency can be written as:
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where 
[image: image229.wmf]a

 is the ratio between the aperture diameter and the Gaussian beam (1 / e2) diameter of the transmit signal, 
[image: image230.wmf]g

 is the obscuration ratio (darkening ratio) and S is the Strehl ratio, which is defined as the intensity at the center of the aberrated system to that of an ideal optical system. 
Optical-Receiver Sensitivity

In addition to the effective delivery of the signal to the detector, the performance of the optical link also depends on the receiver sensitivity (measured in terms of received photons per bit). Because of the high cost associated with increasing the transmit power and system aperture, improving the receiver sensitivity is an important factor

In a direct-detection receiver, the received optical intensity is detected without extensive front-end optical processing. 

[image: image231.emf]
The incident signal is collected by the receive telescope. A polarization filter followed by a narrowband filter, and a field stop effectively reduces the amount of background noise incident onto the detector.

The capacity of a direct detention optical channel in the presence of background can be written as:
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Photon Detection Sensitivity
Improving the photon detection efficiency is an obvious method of improving the channel performance. For a direct-detection receiver, this is generally accomplished by using detectors with internal amplifications, such as avalanche photodiodes (APDs) and photomultiplier tubes (PMTs).

Modulation Format
One practical modulation format to achieve high peak-to-average-power ratio is the M-ary pulse-position modulation (PPM). In an M-ary PPM modulation scheme, each channel symbol period is divided into M time slots, and the information is conveyed through the channel by the time window in which the signal pulse is present.

Link Availability

The communications link budget or the DCT is a useful tool in estimatingthe physical layer link performance (e.g., the link bit error rate). An operational communications link, on the other hand, must also address the issue of link availability. Overall link availability is aimed at >90 percent depending on the link type. In some links, 99.999 % availability may be required.  
Beam Pointing and Tracking

Due to the narrow transmit beamwidth, accurate pointing acquisition and tracking are critical to the deep-space laser communications system implementation.
Typical design parameters considered in an FSO link design:

	Link Budget 
	Parameters

	 
	 

	Received signal power 
	Operating wavelength

	
	Link distance

	
	Transmit power

	
	Transmit aperture area

	
	Transmit optics efficiency

	
	Transmit Strehl ratio

	
	Transmit pointing loss

	
	Polarization mismatch loss

	
	Receiver aperture area

	
	Receive optics efficiency

	
	Receiver detector field of view

	
	Receiver pointing loss

	
	Atmospheric attenuation loss

	
	Scintillation-induced loss

	
	

	Received background power 
	Receive aperture area

	
	Receive optics efficiency

	
	Detector field of view

	
	Receive optical bandwidth

	
	Background spectral irradiance

	
	Receive optics scattering behavior

	
	Detector dark count

	
	

	Receiver sensitivity 
	Detector quantum efficiency

	
	Detector noise characteristics

	
	• Dark count rate or

	
	• Detector Excess and thermal noise

	
	Modulation format

	
	Coding scheme


Direct Detection System

[image: image233.emf]
Block diagram of a direct detection scheme

In direct detection technique, the received optical signal is passed through optical band-pass filter to restrict the background radiation. 

It is then allowed to fall on the photodetector which produces the output electrical signal proportional to the instantaneous intensity of the received optical signal. 

It may be regarded as linear intensity to current convertor or quadratic (square law) converter of optical electric field to detector current. 

The photodetector is followed by an electrical low-pass filter (LPF) with bandwidth sufficient enough to pass the information signal.

The signal-to-noise ratio (SNR) of direct detection receiver can be obtained by using noise models for a particular detector, i.e., PIN or avalanche photodetector (APD). 

With the received power as given above by 
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and detector  noise sources, the SNR expressions are obtained for PIN photodetector to be
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where B is the receiver bandwidth, Id  is the dark current, KB=1.3807 x 10 -23 joules per kelvin (J·K -1) is the Boltzmann’s constant, T is the absolute temperature, RL is the equivalent load resistance, PB is the background noise power and 
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  in mA/watt is the detector responsivity given by
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where 
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 is the detector quantum efficiency, 
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 Coulomb is the electronic charge, 
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 Joule.sec is the Planck’s constant, 
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 the operating frequency. 
When APD is used, the dark current and shot noise are increased by the multiplication process; however, the thermal noise remains unaffected. Therefore, if the photocurrent is increased by a factor of 
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 avalanche multiplication factor, then the total shot noise is also increased by the same factor. For the surface dark current  Ids=0, the direct detection SNR for APD photodetector is
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where F is the excess noise factor arising due to random nature of multiplication factor, Idb is the bulk dark current.
Since the photodetector response is insensitive to the frequency, phase, or polarization of the carrier, this type of receiver is useful only for intensity-modulated signals.
13.  Optical Wireless Communication in Underwater Medium
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Optical wireless communications are a relatively new technology providing many serious advantages, such as the very high rates of data transmission, secure links, very small and light.
Optical waves in the visible spectrum (400–700 nm) present an alternative way to provide broadband communications in the water. They propagate faster in water (300,000,000 m/s) than the acoustic ones (340 m/s in air, 1500 m/s in water), which is about 200,000 times faster than sound travels through water. That is the main reason why they have gained a considerable interest during the last years to serve as a broadband (10–100 Mbps), safe (non-interceptable) and reliable complement to acoustic underwater communications systems.

In general, optical signals are highly absorbed in water, and this is one of the main disadvantages; the other one is the optical scattering by all the particles existing inside the sea. However, seawater shows a decreased absorption in the blue/green region of the visible spectrum. Thus, using suitable wavelengths, for instance in the blue/green region, high speed connections can be attained according to the type of water (400–500 nm for clear to 300–700 nm for turbid water conditions). Minimum attenuation is centered near 0.460 μm in clear waters and shifts to higher values for dirty waters approaching 0.540 μm for coastal waters.
The power received P(z), given initial power P0, propagating through a medium of thickness z is estimated by the Beer’s Law given by
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where 
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 in m-1 is the extinction coefficient expressing the total attenuation occurred by the propagation through the water. 

The total attenuation can be described as the sum of absorption and scattering. Thus,
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where 
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 is the absorption coefficient, 
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 is the scattering coefficient and the product cz is the attenuation length, and it contributes on the reduction of the received power by a factor of exp(-1), or ~63%. 

Beer’s Law provides a limited applicability as it describes only the attenuation due to absorption and single scattering events. In reality, however, many cases of multiple scattering may occur. Also it presumes that the source and receiver are in exact alignment with each other, and it can be applied only in Line-of-Sight (LOS) communication scenarios. Moreover, Beer’s Law ignores temporal dispersion.

More accurate expressions have to take the link geometry into account. For instance, assuming that the transmitter and receiver are positioned in a non LOS configuration, the received power dependent on time t, lateral displacement from the beam axis r, and range z is 
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where 
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 is the transmitted power, 
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 is the aperture and divergence of the optical source, and 
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 is the photoreceiver aperture and field of view. The channel loss term, 
[image: image254.wmf](

)

,,

w

Ltrz

, characterizes the spatial and temporal characteristics of light propagation in seawater.

UOWC propagation 

Underwater medium characteristics

Underwater medium contains almost 80 different elements, dissolved or suspended in pure water, with different concentrations. Some of them are 

• Various dissolved salts such as NaCl, MgCl2, etc, which absorb light at specific wavelengths and induce scattering effects.

• Minerals like sand, metal oxides, which contribute to both absorption and scattering.

• Colored dissolved organic matters such as fulvic and humic acids which affect absorption, mainly in blue and ultraviolet wavelengths.

• Organic matters such as viruses, bacteria, and organic detritus which add backscattering, especially in the blue spectral range.

• Phytoplankton with chlorophyll-A which strongly absorbs in the blue-red region and scatters green light.

Since chlorophyll absorbs the blue and red wavelengths and the particles strongly contribute to the scattering coefficient, we can use its concentration C (in mg/m3) as the free parameter to calculate the absorption and scattering coefficients.

The exact type of water plays a significant role in the estimation of the amount of chlorophyll concentration and consequently the amount of absorption and scattering for a specific geographic location. A classification system for the clarity of water types based on their spectral optical attenuation depth was proposed by Jerlov.

The four major water types are

• Pure deep ocean waters cobalt blue where the absorption is high and the scattering coefficient is low.

• Clear sea waters with higher scattering due to many dissolved particles.

• Near coasts ocean waters with absorption and scattering due to planktonic matters, detritus and mineral components.

• Harbor murky waters, which are quite constraining for optical propagation due to dissolved and in-suspension matters.

Absorption

The absorption coefficient, 
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 is the ratio of the absorbed energy from an incident power per unit distance due to various dissolved particles such as phytoplankton, detritus, etc. 
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where 
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 is the absorption by the pure water in m-1, λ is the wavelength in nm, 
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 is the absorption coefficient of chlorophyll in m-1, 
[image: image259.wmf]c

C

 is the total concentration of chlorophyll per cubic meter (
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 = 35.959 m2/mg is the absorption coefficient of fulvic acid, 
[image: image262.wmf]f

k

= 0.0189 nm-1, 
[image: image263.wmf]f

C

= 0.0189 nm-1, 
[image: image264.wmf]0

h

a

= 18.828 m2/mg is the absorption coefficient of humic acid and 
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 are expressed as
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Scattering

Scattering coefficient, 
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 is the ratio of energy scattered from an incident power per unit distance. It is the sum of backward scattering, 
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Scattering is caused by small and large particles. Small particles are the particles with refractive index equal to 1.15, whereas large particles have a refractive index of 1.03. The scattering and backscattering coefficients are 
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For small and large particulate matter
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and the concentrations are 
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Oceanic turbulence

Optical wireless communications are greatly affected by optical turbulence, which refers to random fluctuations of the refraction index. 
In the case of underwater systems, these fluctuations are mainly caused by variations in temperature and salinity of the oceanic water.

An important parameter for the description of oceanic turbulence is the scintillation index, which expresses the variance of the wave intensity.
Link budget 

Empirical path loss models are effective enough to estimate the received optical power for underwater communications under LOS conditions. 
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where 
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 is the transmitted power, 
[image: image281.wmf]t

h

 and 
[image: image282.wmf]r

h

 are the optical efficiencies of the Tx and Rx correspondingly, 
[image: image283.wmf](

)

c

l

 is the extinction coefficient, R is the perpendicular distance between the Tx plane and the Rx plane, θ0 is the Tx beam divergence angle, θ is the angle between the perpendicular to the Rx plane and the Tx-Rx trajectory, and AR is the receiver aperture area.
14.  All Optical Networking

All optical networks aim at very high data rates in the overall telecommunication network by replacing all the network elements by optical elements. 
· High-capacity telecommunications networks.

· Based on all optical components. 

· All the network is to be designed with all optical elements, thus bandwidth will not be a limiting factor since opto electronic conversions will not be needed throughout the network. 

General considerations in all optical networks:

Electro/Optics and Opto/electronic conversions limit the use of optical network advantage in very high data bit rates because electronics can not handle very high data rates as the optics can handle.

Without optical Add-Drop Multiplexers, each location that demultiplexes signals will need an electrical network element for each channel, even if no traffic is dropping at that site.

By implementing an optical network, only those wavelengths that add or drop traffic at a site need corresponding electrical nodes. Other channels can simply pass through optically, which provides tremendous cost savings in equipment and network management. 

In addition, performing space and wavelength routing of traffic avoids the high cost of electronic cross-connects. 

Wavelength Services: In optical networks, service providers are able to resell bandwidth rather than fiber. By maximizing capacity available on a fiber, service providers can improve revenue by selling wavelengths, regardless of the data rate required. To customers, this service provides the same bandwidth as a dedicated fiber.

Currently employed optical elements in the telecommunications network:

· Optical fibers: 

     First, more capacity between two sites meant the installation of more fibers.

Then more time division multiplexed (TDM) signals are placed in the same fiber, i.e. the bandwith handling capability of the fibers were increased. (both through fiber manufacturing and semiconductor laser modulation techniques supporting high rates of 40 Gbps.)

· Optical networks with Dense Wavelength Division Multiplexing (DWDM) provide additional capacity on existing fibers. DWDM is introduced providing many virtual fibers on a single physical fiber which increased drastically the information rate carrying capability of fibers (in the order of hundreds of Terabits per second).  
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    -   ITU Channel Spacing is shown below:
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    -   Two basic types of DWDM:

i. Unidirectional:  All the wavelengths travel in the same direction on the fiber
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ii. Bidirectional: Signals are split into separate bands, with both bands traveling in different directions. 
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· SDH/SONET. 

· Optical Amplifiers 

· Erbium-Doped Fiber Amplifier (EDFA). By doping a small strand of fiber with a rare earth metal, such as erbium, optical signals could be amplified without converting the signal back to an electrical state. 

· EDFA operating at 1550 nm is used at each 50 – 100 km and replaces electronic regenerators. 

· EDFA enables data rates of 10 Gbps or higher. With the electronic conversion the rate was limited by 2.5 Gbps.  

· Laser diodes used in optical fiber communications.

· LED light sources.

· Optical detectors used in optical fiber communications.

· Tunable Lasers: 

 Radiate light at different wavelengths.

 Can switch from one wavelength to another very quickly.  

· Narrowband Lasers 

Advanced lasers have extremely narrow source spectral bandwidths (<< 1 nm), very narrow wavelength spacings.

Long-haul applications use externally modulated lasers, while shorter applications can use integrated laser technologies. 

Optical elements that are not yet currently employed in the telecommunications network:
· Optical Switches (Sometimes referred to as Optical Cross Connects or Wavelength Routers)
Switch takes traffic in electrical form from an input port or connection and directs it again in electrical form over a backplane, to an output port.

Electronic switches direct variable-length packets, fixed-length cells, and synchronous timeslots from an input port to an output port.

An electronic space switching is shown below:
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An optical switch works with light. It directs a light beam of a single wavelength or of a range of wavelengths from an input port to an output port. 

An optical space switching is shown below:
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A switch needs some kind of information to make the switching decision. In electronic switches, this information is carried inside packets. 

An IP switch, or router, uses the destination IP address (IPD) to make its decision.

The criterion of the optical switch for making a forwarding decision is carried in the so called digital wrapper around each input wavelength of the light.

Wrapper is equivalent to packet header which carries information such as what type of traffic is in the wavelength, where the traffic is headed, ... etc.

As the wavelength moves around the network, the nodes read the wrapper and get the information for originating and terminating details, whether it carries an IP or ATM or another protocol signal, commands such as error correction and whether the wavelength needs to be rerouted.  

Types of Optical Switches:

· MEMS (Micro Electro Mechanical System) Switches: 

Light in one fiber is just redirected  to move to a different fiber by using microscopic (with diameters of a human hair)  moveable (moveable in three dimensions) mirrors (several hundred mirrors placed together on mirror arrays in an area of a few centimeters square). 

Light from an input fiber is aimed at a mirror, which is directed to move the light to another mirror on a facing array. 

Light beams themselves tell the mirror (through digital wrappers) what bend to make in order to route the light appropriately.

This mirror then reflects the light down towards the desired output optical fiber.

There exists designs of 1,024 x 1,024 wavelengths (if each can carry 40 Gbps it corresponds to a capacity of 40 Gbps x 1,024 = 40.96 Tbps) in an area of around 25 cm x 15 cm. 

Picture of a MEMS mirror and MEMS mirror array deflection mechanism are shown below:
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· Buble Switches: Use heat to create small bubles in fluid channels which then reflect and direct light  

· Thermo-optical Switches: 

Light passing through glass is heated up or cooled down by using electrical coils. 

Heat alters the refractive index of the glass, bending the light to enter one fiber or another.  

· Liquid Crystal (LCD) Switches: 

Use liquid to bend light  

       
[image: image291.png]Voltage =0 Bearn Displacer

Polarized Light Q
A
P’
Vottage
Polarized Light Q
A
P’

Liquid Crystal Cell




      Wavelength Switching: 

Single wavelength enters the switch

A “wavelength” selection is made by using prisms, filters or gratings.

Based on the wavelength selected, the light is switched to a known output port.

· Optical Burst Switching: 

Disadvantage of lambda switching is that, once a wavelength has been assigned, it is used exclusively by its “owner.” 

If 100 percent of its capacity is not in use for 100 percent of the time, then there is an inefficiency in the network.

A solution to this is to allocate the wavelength for the duration of the data burst being sent giving rise to optical burst switching.

· Optical Packet Switching (OPS): 

OPS is the optical equivalent of an electronic packet switch, reading the embedded label and making a switching decision using this information.

· Holographic Switching: 

· Creates a wavelength-specific reflective grating, but does this dynamically. 

· The grating structure in these devices is written as a hologram into a piece of glass. 

· The holograms are “invisible” until they are energized by a set of control electrodes.

           
[image: image292.png]Electrode causes hologram
of Bragg Grating to appear | convolsctoces

— ) —

FIRER ( ( 3l ) Feer
Apiece ofglass
RED — < YELLOW
[This grating is This grating is
selective for RED selective for YELLOW
wavelength wavelength

Holographic Switches





· Optical Add/Drop Multiplexers

      Fiber Bragg Gratings
· It is a small section of fiber modified to create periodic changes in the index of refraction. 

· Depending on the space between the changes, a certain frequency of light - the Bragg resonance wavelength - is reflected back, while all other wavelengths pass through. 
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· Optical filters: Fiber Bragg gratings are also used in signal filtering. 

· Multiplexers, demultiplexers

      Thin Film Substrates 
· By coating a thin glass or polymer substrate with a thin interference film of dielectric material, the substrate can be made to pass through only a specific wavelength and reflect all others. 

· By integrating several of these components, optical network devices such as multiplexers, demultiplexers and add/drop devices are designed.
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